;***************************************************************************************
;
; Name      : sprdadb.inf  
;
; Function  : Install UNISOC Android Debug Bridge Driver
;
; Copyright (c) UNISOC Communications Inc.  All rights reserved.
;
;***************************************************************************************

[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %SPRD%
DriverVer  			= 09/30/2021,4.21.39.134
CatalogFile.NTx86   = sprdadb.cat
CatalogFile.NTamd64 = sprdadb.cat
CatalogFile=sprdadb.cat

;
; This section seems to be required for WinUsb driver installation.
; If this section is removed the installer will report an error
; "Required section not found in INF file".
;
[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1

[Manufacturer]
%SPRD% = SPRD, NTx86, NTamd64

[SPRD.NTx86]
; SPRD Adb
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4002&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4003&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4004&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4012&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4013&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4015&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4022&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4023&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4026&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4028&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4029&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4030&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4032&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4033&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4034&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4036&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4037&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4038&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4039&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4040&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4041&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4042&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4044&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4046&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4047&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4048&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4050&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4051&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4052&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4054&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4055&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4061&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4062&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4063&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4064&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4065&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4066&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4067&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4068&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4069&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4070&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4071&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4072&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4073&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4074&MI_09
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4075&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4076&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4077&MI_09
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4078&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4079&MI_09
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4080&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4081&MI_09
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4082&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4083&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4084&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4085&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4086&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4087&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4088&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4089&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4090&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4091&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4092&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4093&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4094&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4095&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4096&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4097&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4098&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4099&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4100&MI_0C
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4101&MI_0C
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4102&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4103&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4104&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4105&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4106&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4107&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4110&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4112&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4D01&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4EE0
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5A5B&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D01&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D04&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D06&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D07&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D21&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D23&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D24&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D25&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D27&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D29&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D31&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D34&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D37&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D38&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D39&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_6000&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A002&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A002&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A012&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A012&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A022&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A022&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_AD21&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_AD21&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_AD24&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_AD24&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D001
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D002
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D003&MI_00
; GOOGLE Adb
%SingleBootLoaderInterface%  = USB_Install, USB\VID_18D1&PID_0FFF
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D06&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D07&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D08&MI_01
%SingleBootLoaderInterface%  = USB_Install, USB\VID_18D1&PID_4EE0
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_4EE7&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_4EE8&MI_00

[SPRD.NTamd64]
; SPRD Adb
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4002&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4003&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4004&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4012&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4013&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4015&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4022&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4023&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4026&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4028&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4029&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4030&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4032&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4033&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4034&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4036&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4037&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4038&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4039&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4040&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4041&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4042&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4044&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4046&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4047&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4048&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4050&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4051&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4052&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4054&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4055&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4061&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4062&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4063&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4064&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4065&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4066&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4067&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4068&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4069&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4070&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4071&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4072&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4073&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4074&MI_09
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4075&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4076&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4077&MI_09
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4078&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4079&MI_09
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4080&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4081&MI_09
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4082&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4083&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4084&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4085&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4086&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4087&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4088&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4089&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4090&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4091&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4092&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4093&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4094&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4095&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4096&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4097&MI_07
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4098&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4099&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4100&MI_0C
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4101&MI_0C
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4102&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4103&MI_0A
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4104&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4105&MI_08
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4106&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4107&MI_06
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4110&MI_05
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4112&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4D01&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4EE0
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5A5B&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D01&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D04&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D06&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D07&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D21&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D23&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D24&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D25&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D27&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D29&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D31&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D34&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D37&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D38&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D39&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_6000&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A002&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A002&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A012&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A012&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A022&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A022&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_AD21&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_AD21&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_AD24&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_AD24&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D001
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D002
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D003&MI_00
; GOOGLE Adb
%SingleBootLoaderInterface%  = USB_Install, USB\VID_18D1&PID_0FFF
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D06&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D07&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D08&MI_01
%SingleBootLoaderInterface%  = USB_Install, USB\VID_18D1&PID_4EE0
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_4EE7&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_4EE8&MI_00

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion  = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
SPRD                        = "UNISOC Communications Inc."
SingleAdbInterface          = "Android ADB Interface"
CompositeAdbInterface       = "Android Composite ADB Interface"
CompositeAdbInterface2      = "Android Composite YDB Interface"
SingleBootLoaderInterface   = "Android Bootloader&ADB Interface"
WinUSB_SvcDesc              = "Android USB Driver"
DISK_NAME                   = "Android WinUsb installation disk"
ClassName                   = "Android Phone"
