;***************************************************************************************
;
; Name      : sprdvmdm.inf  
;
; Function  : Install UNISOC USB Modem Driver
;
; Copyright (c) UNISOC Communications Inc.  All rights reserved.
;
;***************************************************************************************


[Version]
Signature   = "$WINDOWS NT$"
Class       = Modem
Provider    = %SPRD%
ClassGuid   = {4D36E96D-E325-11CE-BFC1-08002BE10318}
DriverVer   = 09/30/2021,4.21.39.134
CatalogFile =sprdvmdm.cat

[ControlFlags]
ExcludeFromSelect = *

[SourceDisksNames]
1 = %SRCDISK%,,,\i386
2 = %SRCDISK%,,,\amd64

[SourceDisksFiles.x86]
sprdvmdm.sys             = 1
WdfCoInstaller01009.dll  = 1

[SourceDisksFiles.amd64]
sprdvmdm.sys             = 2
WdfCoInstaller01009.dll  = 2

[DestinationDirs]
DefaultDestDir           = 12
Modem6k.NT.Copy          = 12
CoInstaller_CopyFiles    = 11

[Manufacturer]
%SPRD% = SPRD,NTx86,NTAMD64

[SPRD]
%HSPA_MODEM% = Modem6k, USB\VID_1782&PID_0009&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D00&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D02&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D03&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4026&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4027&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4028&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4029&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4030&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4031&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4032&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4033&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4034&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4035&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4036&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4037&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4038&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4039&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4040&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4041&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4044&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4045&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4046&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4047&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4048&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4049&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4050&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4051&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4052&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4053&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4054&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4055&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4056&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4057&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4058&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4059&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4061&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4062&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4063&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4064&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4065&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4066&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4067&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4068&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4069&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4073&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4074&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4075&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4076&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4077&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4078&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4079&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4080&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4081&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4085&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4086&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4087&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4100&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4101&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4102&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4103&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4104&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4105&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4106&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4107&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4108&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4109&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410A&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410B&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410C&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410D&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410E&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410F&MI_05

; LSD add start
%LSD_modem% = Modem6k, USB\VID_3505&PID_1001&MI_05
%LSD_modem% = Modem6k, USB\VID_3505&PID_1002&MI_05
; LSD add end
; LSD EC618/EC718
%LCAT1_modem% = Modem6k, USB\Class_ff&SubClass_00&Prot_05
; LSD add end


[SPRD.NTx86]
%HSPA_MODEM% = Modem6k, USB\VID_1782&PID_0009&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D00&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D02&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D03&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4026&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4027&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4028&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4029&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4030&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4031&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4032&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4033&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4034&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4035&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4036&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4037&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4038&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4039&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4040&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4041&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4044&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4045&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4046&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4047&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4048&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4049&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4050&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4051&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4052&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4053&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4054&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4055&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4056&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4057&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4058&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4059&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4061&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4062&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4063&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4064&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4065&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4066&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4067&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4068&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4069&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4073&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4074&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4075&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4076&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4077&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4078&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4079&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4080&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4081&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4085&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4086&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4087&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4100&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4101&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4102&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4103&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4104&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4105&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4106&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4107&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4108&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4109&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410A&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410B&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410C&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410D&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410E&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410F&MI_05

; LSD add start
%LSD_modem% = Modem6k, USB\VID_3505&PID_1001&MI_05
%LSD_modem% = Modem6k, USB\VID_3505&PID_1002&MI_05
; LSD add end
; LSD EC618/EC718
%LCAT1_modem% = Modem6k, USB\Class_ff&SubClass_00&Prot_05
; LSD add end

[SPRD.NTAMD64]
%HSPA_MODEM% = Modem6k, USB\VID_1782&PID_0009&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D00&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D02&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_3D03&MI_02
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4026&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4027&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4028&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4029&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4030&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4031&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4032&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4033&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4034&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4035&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4036&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4037&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4038&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4039&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4040&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4041&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4044&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4045&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4046&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4047&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4048&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4049&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4050&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4051&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4052&MI_06
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4053&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4054&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4055&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4056&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4057&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4058&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4059&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4061&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4062&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4063&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4064&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4065&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4066&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4067&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4068&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4069&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4073&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4074&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4075&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4076&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4077&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4078&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4079&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4080&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4081&MI_04
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4085&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4086&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4087&MI_03
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4100&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4101&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4102&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4103&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4104&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4105&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4106&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4107&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4108&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_4109&MI_0B
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410A&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410B&MI_09
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410C&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410D&MI_07
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410E&MI_05
%SPRD_MODEM% = Modem6k, USB\VID_1782&PID_410F&MI_05

; LSD add start
%LSD_modem% = Modem6k, USB\VID_3505&PID_1001&MI_05
%LSD_modem% = Modem6k, USB\VID_3505&PID_1002&MI_05

; LSD EC618/EC718
%LCAT1_modem% = Modem6k, USB\Class_ff&SubClass_00&Prot_05
; LSD add end



[Modem6k.NT]
CopyFiles = Modem6k.NT.Copy
AddReg    = All, MfgAddReg, Modem1.AddReg, USB

[Modem6k.NT.Services]
AddService = sprdvmdm, 0x00000000, LowerFilter_Service_Inst6k

[Modem6k.NT.HW]
AddReg     = LowerFilterAddReg6k

[Modem6k.NT.Copy]
sprdvmdm.sys,,,0x06

[LowerFilterAddReg6k]
HKR,,"LowerFilters",0x00010000,"sprdvmdm"
HKR,,DeviceCharacteristics,0x10001,0x0100         ; Use same security checks on relative opens
HKR,,Security,,"D:P(A;;GA;;;BA)(A;;GA;;;WD)"      ; Allow generic-all access to Built-in administrators and Local system 
HKR,,"VendorRequestTimeoutValue", %REG_DWORD%,5
HKR,,"SprdVendorRequest",%REG_DWORD%,1            ; If SprdVendorRequest is 1, CdcControlLineState will be ignored
HKR,,"CdcControlLineState",%REG_DWORD%,0          ; Only if SprdVendorRequest is 0, this configure will be worked
HKR,,"UseContinuousRead",%REG_DWORD%,0
HKR,,"RxFifoSize",%REG_DWORD%,128                 ; KByte
HKR,,"BulkInBufSize",%REG_DWORD%,4                ; KByte
HKR,,"UsbEnableZLP",%REG_DWORD%,1

[LowerFilter_Service_Inst6k]
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\sprdvmdm.sys
AddReg        = Service_AddReg

[Service_AddReg]
HKR,,TraceFile,%REG_DWORD%,1

;-------------- WDF Coinstaller installation

[Modem6k.NT.CoInstallers]
AddReg     = CoInstaller_AddReg
CopyFiles  = CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
WdfCoInstaller01009.dll

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[Modem6k.NT.Wdf]
KmdfService = sprdvmdm, Serial_wdfsect

[Serial_wdfsect]
KmdfLibraryVersion = 1.9

[Strings]
SPRD          = "UNISOC Communications Inc"
SRCDISK       = "UNISOC Virtual Modem Installation Disk"
HSPA_MODEM    = "SPRD HSPA Modem"
SPRD_MODEM    = "SPRD Modem"
REG_EXPAND_SZ = 0x00020000
REG_DWORD     = 0x00010001

; LSD add start
LSD_modem = "LSD USB Modem"

LCAT1_modem = "Lierda USB Modem"
; LSD add end



[All]
HKR,,FriendlyDriver,0,Unimodem.vxd
HKR,,DevLoader,0,*vcomm
HKR,,ConfigDialog,0,modemui.dll
HKR,,EnumPropPages,0,modemui.dll,EnumPropPages
HKR,,PortSubClass,1,02
HKR, Init,      1,, "AT<cr>"
HKR,,InitialBaudRate, 0x10001, 00,DD,6D,00			;7.2M initial baud rate
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit

[Modem1.AddReg]
HKR,,Properties,  1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 31,00,00,00, 00,40,1F,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,dd,6d,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,, FClass, 1, c3,00,00,00
HKR, Fax, CL1FCS,, "2"
HKR, Fax, HardwareFlowControl,, "1"

[USB]
HKR,, DeviceType, 1, 01
HKR,,Contention,,""

[MfgAddReg]
HKR,, InactivityScale,1, 3c,00,00,00
HKR, Init,    1,, "AT<cr>"
HKR, Init, 2,, "ATE0V1<cr>"
;HKR, Init,    2,, "ATV1<cr>"
;HKR, Init,    3,, "ATE0<cr>"
;HKR, Init,    4,, "AT&F&D2&C1S0=0<cr>"
;HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 1,, "None"
HKR, Answer,    1,, "ATA<cr>"
HKR, Hangup,    1,, "ATH E1<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
;HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
;HKR, Settings, InactivityTimeOut,,"S30=<#>"

HKR, Responses, "0<cr>",                       1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK - Command executed
HKR, Responses, "1<cr>",                       1, 02, 00, 00,00,00,00, 00,00,00,00 ; CONNECT - Connection
HKR, Responses, "2<cr>",                       1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING - Ring signal indicated
HKR, Responses, "3<cr>",                       1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>",                       1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR - Invalid command
HKR, Responses, "5<cr>",                       1, 02, 00, B0,04,00,00, 00,00,00,00 ; CONNECT 1200
HKR, Responses, "6<cr>",                       1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE - No dial tone detected
HKR, Responses, "7<cr>",                       1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY - Engaged (busy) signal
HKR, Responses, "8<cr>",                       1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER
HKR, Responses, "<cr><lf>OK<cr><lf>",          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",             1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>",  1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIAL TONE<cr><lf>",1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",   1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                1, 02, 00, 80,B9,2A,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",       1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",       1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",       1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>",      1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",      1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>",      1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600<cr><lf>",      1, 02, 00, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",      1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",      1, 02, 00, 00,e1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",      1, 02, 00, 00,c2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 8000<cr><lf>",           1, 02, 00, 40,1F,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16000<cr><lf>",          1, 02, 00, 80,3E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000<cr><lf>",          1, 02, 00, 00,7D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000<cr><lf>",      1, 02, 00, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 85600<cr><lf>" , 1, 02, 00, 60,4E,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 128000<cr><lf>",         1, 02, 00, 00,F4,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 144000<cr><lf>",         1, 02, 00, 80,32,02,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 236800<cr><lf>",     1, 02, 00, 00,9D,03,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 256000<cr><lf>",         1, 02, 00, 00,E8,03,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 384000<cr><lf>",         1, 02, 00, 00,DC,05,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 512000<cr><lf>",         1, 02, 00, 00,D0,07,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1024000<cr><lf>",        1, 02, 00, 00,A0,0F,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1536000<cr><lf>",        1, 02, 00, 00,70,17,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2048000<cr><lf>",        1, 02, 00, 00,40,1F,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2800000<cr><lf>", 1, 02, 00, 80,B9,2A,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 3600000<cr><lf>",     1, 02, 00, 80,EE,36,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 3686400<cr><lf>", 1, 02, 00, 00,40,38,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200000<cr><lf>",     1, 02, 00, 00,DD,6D,00, 00,00,00,00
HKR, Responses, "<cr><lf>FAX<cr><lf>",                    1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATA<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>VOICE<cr><lf>",                  1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RINGING<cr><lf>",                1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED<cr><lf>",                1, 1D, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED NUMBER<cr><lf>",         1, 1D, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED<cr><lf>",            1, 1C, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED NUMBER<cr><lf>",     1, 1C, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+FCERROR<cr><lf>",               1, 03, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>+CME ERROR: 0<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Phone failure.
HKR, Responses, "<cr><lf>+CME ERROR: 1<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; No connection to phone.
HKR, Responses, "<cr><lf>+CME ERROR: 2<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Phone modem link reserved.
HKR, Responses, "<cr><lf>+CME ERROR: 3<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Operation not permitted.
HKR, Responses, "<cr><lf>+CME ERROR: 4<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Operation not supported.
HKR, Responses, "<cr><lf>+CME ERROR: 5<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; PH-SIM card PIN required.
HKR, Responses, "<cr><lf>+CME ERROR: 6<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; PH-FSIM PIN required
HKR, Responses, "<cr><lf>+CME ERROR: 7<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; PH-FSIM PUK required
HKR, Responses, "<cr><lf>+CME ERROR: 10<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card not inserted.
HKR, Responses, "<cr><lf>+CME ERROR: 11<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card PIN required.
HKR, Responses, "<cr><lf>+CME ERROR: 12<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card PUK required.
HKR, Responses, "<cr><lf>+CME ERROR: 13<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card failure.
HKR, Responses, "<cr><lf>+CME ERROR: 14<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card busy.
HKR, Responses, "<cr><lf>+CME ERROR: 15<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card wrong.
HKR, Responses, "<cr><lf>+CME ERROR: 16<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Incorrect password.
HKR, Responses, "<cr><lf>+CME ERROR: 20<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Memory full.
HKR, Responses, "<cr><lf>+CME ERROR: 21<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid index.
HKR, Responses, "<cr><lf>+CME ERROR: 22<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Not found.
HKR, Responses, "<cr><lf>+CME ERROR: 23<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Memory failure.
HKR, Responses, "<cr><lf>+CME ERROR: 24<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Text string too long.
HKR, Responses, "<cr><lf>+CME ERROR: 25<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid character in text string.
HKR, Responses, "<cr><lf>+CME ERROR: 26<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Dial string too long.
HKR, Responses, "<cr><lf>+CME ERROR: 27<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid character in dial string.
HKR, Responses, "<cr><lf>+CME ERROR: 30<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; No network service
HKR, Responses, "<cr><lf>+CME ERROR: 31<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Network timeout
HKR, Responses, "<cr><lf>+CME ERROR: 100<cr><lf>",  1, 03, 00, 00,00,00,00, 00,00,00,00   ; Unknown.
HKR, Responses, "<cr><lf>+CMS ERROR: ",             1, 03, 00, 00,00,00,00, 00,00,00,00   ; CMS errors
