;***************************************************************************************
;
; Name      : sprdvcom.inf  
;
; Function  : Install UNISOC USB Serial Driver
;
; Copyright (c) UNISOC Communications Inc.  All rights reserved.
;
;***************************************************************************************

[version]
signature   = "$CHICAGO$"
Class       = Ports
ClassGuid   = {4D36E978-E325-11CE-BFC1-08002BE10318}
Provider    = %SPRD%
DriverVer   = 09/30/2021,4.21.39.134
CatalogFile =sprdvcom.cat

; ================= Device Install section =====================

[ControlFlags]
ExcludeFromSelect=*

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WdfCoInstaller01009.dll = 1
sprdvcom.sys            = 1

[SourceDisksFiles.amd64]
WdfCoInstaller01009.dll = 2
sprdvcom.sys            = 2

[DestinationDirs]
DefaultDestDir          = 12
CoInstaller_CopyFiles   = 11

[Manufacturer]
%SPRD% = SPRD,NTx86,NTAMD64

[SPRD]
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_0009&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_0009&MI_01
%SPRD.AT2%    = Serial_Inst, USB\VID_1782&PID_0009&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000A&MI_02
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000A&MI_03
%SPRD.CM4LOG% = Serial_Inst, USB\VID_1782&PID_000A&MI_04
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_000A&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000B&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000B&MI_01
%SPRD.CM4LOG% = Serial_Inst, USB\VID_1782&PID_000B&MI_02
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_000B&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000C&MI_02
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000C&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D00&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D00&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D01&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D01&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D02&MI_01

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D03&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D03&MI_00
%SPRD.CPLOG%  = Serial_Inst, USB\VID_1782&PID_3D03&MI_03

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D10&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D13

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4001&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4001&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4001&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4001&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4001&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4001&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4002&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4002&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4002&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4002&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4002&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4002&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4003&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4003&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4003&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4004&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4004&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4004&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4004&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4004&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4004&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4012&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4012&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4012&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4012&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4012&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4012&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4013&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4013&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4013&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4015&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4015&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4015&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4015&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4015&MI_09


%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4022&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4022&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4022&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4022&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4022&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4022&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4023&MI_03
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4023&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4023&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4024&MI_00
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_01
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4024&MI_02
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4024&MI_03
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_04
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4024&MI_05
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_06
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4024&MI_07

;%SPRD.DIAG%  = Serial_Inst, USB\VID_1782&PID_4025&MI_03
;%SPRD.LOG%   = Serial_Inst, USB\VID_1782&PID_4025&MI_04
;%SPRD.AT%    = Serial_Inst, USB\VID_1782&PID_4025&MI_05

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4026&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4026&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4026&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4027&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4027&MI_03
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4027&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4028&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4028&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4029&MI_02

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4030&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4030&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4030&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4031&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4031&MI_03
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4031&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4032&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4032&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4033&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4034&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4034&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4034&MI_05

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4035&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4035&MI_03
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4035&MI_05

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4036&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4036&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4037&MI_02

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4038&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4038&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4038&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4039&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4039&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4039&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4040&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4040&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4040&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4041&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4041&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4041&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_09

%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_08


%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4044&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4044&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4044&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4044&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4044&MI_08

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4045&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4045&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4045&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4045&MI_06
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4045&MI_07

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4046&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4046&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4046&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4046&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4047&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4047&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4047&MI_05

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4048&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4048&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4048&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4048&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4048&MI_08

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4049&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4049&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4049&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4049&MI_06
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4049&MI_07

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4050&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4050&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4050&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4050&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4051&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4051&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4051&MI_05

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4052&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4052&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4052&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4052&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4052&MI_08

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4053&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4053&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4053&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4053&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4053&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4054&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4054&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4054&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4054&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4055&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4055&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4055&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4056&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4056&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4056&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4057&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4057&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4057&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4058&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4058&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4058&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4059&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4059&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4059&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_08

%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4061&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4061&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4061&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4061&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4061&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4062&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4062&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4062&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4062&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4063&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4063&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4063&MI_05

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4064&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4064&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4064&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4064&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4064&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4065&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4065&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4065&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4065&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4066&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4066&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4066&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4066&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4066&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4067&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4067&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4067&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4067&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4068&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4068&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4068&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4068&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4068&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4069&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4069&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4069&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4069&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4070&MI_00
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4070&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4070&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4070&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4070&MI_04

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4071&MI_00
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4071&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4071&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4071&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4072&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4072&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4072&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4073&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4073&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4073&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4073&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4073&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4073&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4073&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4074&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4074&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4074&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4074&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4074&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4074&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4075&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4075&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4075&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4075&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4075&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4076&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4076&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4076&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4076&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4076&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4076&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4076&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4077&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4077&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4077&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4077&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4077&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4077&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4078&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4078&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4078&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4078&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4078&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4078&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4078&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4079&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4079&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4079&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4079&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4079&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4079&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4080&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4080&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4080&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4080&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4080&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4080&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4080&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4081&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4081&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4081&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4081&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4081&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4081&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4082&MI_00
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4082&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4082&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4082&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4082&MI_04
%WCN.AT%        = Serial_Inst, USB\VID_1782&PID_4082&MI_05
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4082&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4083&MI_00
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4083&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4083&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4083&MI_03
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4083&MI_04
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4083&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4084&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4084&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4084&MI_02
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4084&MI_03
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4084&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4085&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4085&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4085&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4085&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4085&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4086&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4086&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4086&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4086&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4086&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4087&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4087&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4087&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4087&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4087&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4088&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4088&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4088&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4088&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4088&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4089&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4089&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4089&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4089&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4090&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4090&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4090&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4091&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4091&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4091&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4091&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4091&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4092&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4092&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4092&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4092&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4093&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4093&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4093&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4094&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4094&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4094&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4094&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4094&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4095&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4095&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4095&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4095&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4096&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4096&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4096&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4097&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4097&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4097&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4097&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4097&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4098&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4098&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4098&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4098&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4099&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4099&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4099&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4100&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4100&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4100&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4100&MI_0D

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4101&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4101&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4101&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4101&MI_0D

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4102&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4102&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4102&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4102&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4103&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4103&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4103&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4103&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4104&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4104&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4104&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4104&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4105&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4105&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4105&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4105&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4106&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4106&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4106&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4106&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4107&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4107&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4107&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4107&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4108&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4108&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4108&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4108&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4109&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4109&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4109&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4109&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410A&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410A&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410A&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410A&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410B&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410B&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410B&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410B&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410C&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410C&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410C&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410C&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410D&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410D&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410D&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410D&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410E&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410E&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410E&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410E&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410F&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410F&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410F&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410F&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4110&MI_00
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4110&MI_01
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4110&MI_02
%WCN.AT%       = Serial_Inst, USB\VID_1782&PID_4110&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4110&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4111&MI_00
%WCN.AT%       = Serial_Inst, USB\VID_1782&PID_4111&MI_01
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4111&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4112&MI_00
%SPRD.AT%       = Serial_Inst, USB\VID_1782&PID_4112&MI_01
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4112&MI_02
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4112&MI_03


%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_4D00

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4D01&MI_01
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4D01&MI_02

%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_4D02        ; For RDA

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4D03&MI_00
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4D03&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5A5B&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5A5B&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5A5B&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5A5B&MI_09

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D03&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D03&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D03&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D03&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_09

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D04&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D04&MI_03

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_5D06&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D06&MI_02

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_5D07&MI_01
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_5D07&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D07&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D21&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D21&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D21&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D21&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_0B

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D23&MI_02

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D24&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D24&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D24&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D24&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_0A
;8830ec
%TD.AT%       = Serial_Inst, USB\VID_1782&PID_5D25&MI_03
%TD.DIAG%     = Serial_Inst, USB\VID_1782&PID_5D25&MI_04
%W.AT%        = Serial_Inst, USB\VID_1782&PID_5D25&MI_05
%W.DIAG%      = Serial_Inst, USB\VID_1782&PID_5D25&MI_06
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D25&MI_07
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D25&MI_08
;8830ec
%TD.AT%       = Serial_Inst, USB\VID_1782&PID_5D26&MI_01
%TD.DIAG%     = Serial_Inst, USB\VID_1782&PID_5D26&MI_02
%W.AT%        = Serial_Inst, USB\VID_1782&PID_5D26&MI_03
%W.DIAG%      = Serial_Inst, USB\VID_1782&PID_5D26&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D26&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D26&MI_06
;Dechen8830
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D27&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D27&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D27&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D27&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D28&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D28&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D28&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D28&MI_04

%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_5D29&MI_00

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D31&MI_03
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D31&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D31&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D34&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D34&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D34&MI_04

%CUSPORT%     = Serial_Inst, USB\VID_1782&PID_5D38&MI_00

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_01
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D39&MI_02
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D39&MI_03
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_04
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D39&MI_05
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_06
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D39&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_6000&MI_01
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_6000&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_6000&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A002&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A002&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A002&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A002&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A002&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A002&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A012&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A012&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A012&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A012&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A012&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A012&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A022&MI_04
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_05
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A022&MI_06
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A022&MI_07
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_08
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A022&MI_09
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_0A
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A022&MI_0B
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A022&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_04
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_05
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_AD21&MI_06
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_AD21&MI_07
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_08
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_AD21&MI_09
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_0A
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_AD21&MI_0B
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_AD24&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_AD24&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_AD24&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_AD24&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_D003&MI_01
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_D003&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_D003&MI_03
%CUSPORT%     = Serial_Inst, USB\VID_1782&PID_D003&MI_04

;GOOGLE
%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D06&MI_03
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D06&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D06&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D07&MI_02
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D07&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D07&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D08&MI_02
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D08&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D08&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_05
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_07
%LTELOG%      = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_01
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_03

; LSD add start
%LSD.DIAG%   = Serial_Inst, USB\VID_3505&PID_1001&MI_02
%LSD.LOG%    = Serial_Inst, USB\VID_3505&PID_1001&MI_03
%LSD.AT%     = Serial_Inst, USB\VID_3505&PID_1001&MI_04
%LSD.DIAG%   = Serial_Inst, USB\VID_3505&PID_1002&MI_02
%LSD.LOG%    = Serial_Inst, USB\VID_3505&PID_1002&MI_03
%LSD.AT%     = Serial_Inst, USB\VID_3505&PID_1002&MI_04
%LSD.APLOG%  = Serial_Inst, USB\VID_3505&PID_1002&MI_06

; LCAT1 EC618/EC718
%LCAT1.AT%     = Serial_Inst, USB\Class_ff&SubClass_00&Prot_03
%LCAT1.LOG%    = Serial_Inst, USB\Class_ff&SubClass_00&Prot_04
%LCAT1.OPAQ%   = Serial_Inst, USB\Class_ff&SubClass_00&Prot_06

%LCAT1.QDLOADE% = Serial_Inst, USB\VID_17D1&PID_0001&REV_0200
; LSD add end


; For XP and later
[SPRD.NTx86]
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_0009&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_0009&MI_01
%SPRD.AT2%    = Serial_Inst, USB\VID_1782&PID_0009&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000A&MI_02
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000A&MI_03
%SPRD.CM4LOG% = Serial_Inst, USB\VID_1782&PID_000A&MI_04
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_000A&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000B&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000B&MI_01
%SPRD.CM4LOG% = Serial_Inst, USB\VID_1782&PID_000B&MI_02
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_000B&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000C&MI_02
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000C&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D00&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D00&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D01&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D01&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D02&MI_01

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D03&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D03&MI_00
%SPRD.CPLOG%  = Serial_Inst, USB\VID_1782&PID_3D03&MI_03

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D10&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D13

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4001&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4001&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4001&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4001&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4001&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4001&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4002&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4002&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4002&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4002&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4002&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4002&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4003&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4003&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4003&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4004&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4004&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4004&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4004&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4004&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4004&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4012&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4012&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4012&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4012&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4012&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4012&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4013&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4013&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4013&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4015&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4015&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4015&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4015&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4015&MI_09


%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4022&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4022&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4022&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4022&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4022&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4022&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4023&MI_03
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4023&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4023&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4024&MI_00
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_01
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4024&MI_02
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4024&MI_03
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_04
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4024&MI_05
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_06
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4024&MI_07

;%SPRD.DIAG%  = Serial_Inst, USB\VID_1782&PID_4025&MI_03
;%SPRD.LOG%   = Serial_Inst, USB\VID_1782&PID_4025&MI_04
;%SPRD.AT%    = Serial_Inst, USB\VID_1782&PID_4025&MI_05

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4026&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4026&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4026&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4027&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4027&MI_03
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4027&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4028&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4028&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4029&MI_02

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4030&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4030&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4030&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4031&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4031&MI_03
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4031&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4032&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4032&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4033&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4034&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4034&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4034&MI_05

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4035&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4035&MI_03
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4035&MI_05

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4036&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4036&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4037&MI_02

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4038&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4038&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4038&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4039&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4039&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4039&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4040&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4040&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4040&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4041&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4041&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4041&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_09

%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_08


%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4044&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4044&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4044&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4044&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4044&MI_08

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4045&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4045&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4045&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4045&MI_06
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4045&MI_07

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4046&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4046&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4046&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4046&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4047&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4047&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4047&MI_05

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4048&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4048&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4048&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4048&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4048&MI_08

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4049&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4049&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4049&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4049&MI_06
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4049&MI_07

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4050&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4050&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4050&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4050&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4051&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4051&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4051&MI_05

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4052&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4052&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4052&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4052&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4052&MI_08

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4053&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4053&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4053&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4053&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4053&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4054&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4054&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4054&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4054&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4055&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4055&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4055&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4056&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4056&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4056&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4057&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4057&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4057&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4058&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4058&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4058&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4059&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4059&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4059&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_08

%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4061&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4061&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4061&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4061&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4061&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4062&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4062&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4062&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4062&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4063&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4063&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4063&MI_05

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4064&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4064&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4064&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4064&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4064&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4065&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4065&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4065&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4065&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4066&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4066&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4066&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4066&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4066&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4067&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4067&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4067&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4067&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4068&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4068&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4068&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4068&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4068&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4069&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4069&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4069&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4069&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4070&MI_00
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4070&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4070&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4070&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4070&MI_04

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4071&MI_00
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4071&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4071&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4071&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4072&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4072&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4072&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4073&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4073&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4073&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4073&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4073&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4073&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4073&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4074&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4074&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4074&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4074&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4074&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4074&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4075&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4075&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4075&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4075&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4075&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4076&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4076&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4076&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4076&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4076&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4076&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4076&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4077&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4077&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4077&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4077&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4077&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4077&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4078&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4078&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4078&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4078&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4078&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4078&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4078&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4079&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4079&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4079&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4079&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4079&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4079&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4080&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4080&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4080&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4080&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4080&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4080&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4080&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4081&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4081&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4081&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4081&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4081&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4081&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4082&MI_00
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4082&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4082&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4082&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4082&MI_04
%WCN.AT%        = Serial_Inst, USB\VID_1782&PID_4082&MI_05
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4082&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4083&MI_00
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4083&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4083&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4083&MI_03
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4083&MI_04
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4083&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4084&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4084&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4084&MI_02
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4084&MI_03
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4084&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4085&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4085&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4085&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4085&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4085&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4086&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4086&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4086&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4086&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4086&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4087&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4087&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4087&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4087&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4087&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4088&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4088&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4088&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4088&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4088&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4089&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4089&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4089&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4089&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4090&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4090&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4090&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4091&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4091&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4091&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4091&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4091&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4092&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4092&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4092&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4092&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4093&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4093&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4093&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4094&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4094&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4094&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4094&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4094&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4095&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4095&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4095&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4095&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4096&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4096&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4096&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4097&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4097&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4097&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4097&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4097&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4098&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4098&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4098&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4098&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4099&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4099&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4099&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4100&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4100&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4100&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4100&MI_0D

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4101&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4101&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4101&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4101&MI_0D

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4102&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4102&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4102&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4102&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4103&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4103&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4103&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4103&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4104&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4104&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4104&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4104&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4105&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4105&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4105&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4105&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4106&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4106&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4106&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4106&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4107&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4107&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4107&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4107&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4108&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4108&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4108&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4108&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4109&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4109&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4109&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4109&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410A&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410A&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410A&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410A&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410B&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410B&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410B&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410B&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410C&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410C&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410C&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410C&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410D&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410D&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410D&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410D&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410E&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410E&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410E&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410E&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410F&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410F&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410F&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410F&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4110&MI_00
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4110&MI_01
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4110&MI_02
%WCN.AT%       = Serial_Inst, USB\VID_1782&PID_4110&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4110&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4111&MI_00
%WCN.AT%       = Serial_Inst, USB\VID_1782&PID_4111&MI_01
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4111&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4112&MI_00
%SPRD.AT%       = Serial_Inst, USB\VID_1782&PID_4112&MI_01
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4112&MI_02
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4112&MI_03

%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_4D00

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4D01&MI_01
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4D01&MI_02

%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_4D02        ; For RDA

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4D03&MI_00
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4D03&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5A5B&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5A5B&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5A5B&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5A5B&MI_09

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D03&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D03&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D03&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D03&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_09

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D04&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D04&MI_03

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_5D06&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D06&MI_02

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_5D07&MI_01
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_5D07&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D07&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D21&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D21&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D21&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D21&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_0B

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D23&MI_02

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D24&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D24&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D24&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D24&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_0A
;8830ec
%TD.AT%       = Serial_Inst, USB\VID_1782&PID_5D25&MI_03
%TD.DIAG%     = Serial_Inst, USB\VID_1782&PID_5D25&MI_04
%W.AT%        = Serial_Inst, USB\VID_1782&PID_5D25&MI_05
%W.DIAG%      = Serial_Inst, USB\VID_1782&PID_5D25&MI_06
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D25&MI_07
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D25&MI_08
;8830ec
%TD.AT%       = Serial_Inst, USB\VID_1782&PID_5D26&MI_01
%TD.DIAG%     = Serial_Inst, USB\VID_1782&PID_5D26&MI_02
%W.AT%        = Serial_Inst, USB\VID_1782&PID_5D26&MI_03
%W.DIAG%      = Serial_Inst, USB\VID_1782&PID_5D26&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D26&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D26&MI_06
;Dechen8830
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D27&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D27&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D27&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D27&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D28&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D28&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D28&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D28&MI_04

%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_5D29&MI_00

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D31&MI_03
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D31&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D31&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D34&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D34&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D34&MI_04

%CUSPORT%     = Serial_Inst, USB\VID_1782&PID_5D38&MI_00

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_01
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D39&MI_02
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D39&MI_03
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_04
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D39&MI_05
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_06
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D39&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_6000&MI_01
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_6000&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_6000&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A002&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A002&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A002&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A002&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A002&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A002&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A012&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A012&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A012&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A012&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A012&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A012&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A022&MI_04
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_05
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A022&MI_06
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A022&MI_07
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_08
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A022&MI_09
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_0A
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A022&MI_0B
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A022&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_04
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_05
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_AD21&MI_06
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_AD21&MI_07
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_08
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_AD21&MI_09
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_0A
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_AD21&MI_0B
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_AD24&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_AD24&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_AD24&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_AD24&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_D003&MI_01
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_D003&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_D003&MI_03
%CUSPORT%     = Serial_Inst, USB\VID_1782&PID_D003&MI_04

;GOOGLE
%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D06&MI_03
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D06&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D06&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D07&MI_02
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D07&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D07&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D08&MI_02
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D08&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D08&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_05
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_07
%LTELOG%      = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_01
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_03

; LSD add start
%LSD.DIAG%   = Serial_Inst, USB\VID_3505&PID_1001&MI_02
%LSD.LOG%    = Serial_Inst, USB\VID_3505&PID_1001&MI_03
%LSD.AT%     = Serial_Inst, USB\VID_3505&PID_1001&MI_04
%LSD.DIAG%   = Serial_Inst, USB\VID_3505&PID_1002&MI_02
%LSD.LOG%    = Serial_Inst, USB\VID_3505&PID_1002&MI_03
%LSD.AT%     = Serial_Inst, USB\VID_3505&PID_1002&MI_04
%LSD.APLOG%  = Serial_Inst, USB\VID_3505&PID_1002&MI_06

; LCAT1 EC618/EC718
%LCAT1.AT%     = Serial_Inst, USB\Class_ff&SubClass_00&Prot_03
%LCAT1.LOG%    = Serial_Inst, USB\Class_ff&SubClass_00&Prot_04
%LCAT1.OPAQ%   = Serial_Inst, USB\Class_ff&SubClass_00&Prot_06

%LCAT1.QDLOADE% = Serial_Inst, USB\VID_17D1&PID_0001&REV_0200
; LSD add end


[SPRD.NTAMD64]
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_0009&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_0009&MI_01
%SPRD.AT2%    = Serial_Inst, USB\VID_1782&PID_0009&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000A&MI_02
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000A&MI_03
%SPRD.CM4LOG% = Serial_Inst, USB\VID_1782&PID_000A&MI_04
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_000A&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000B&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000B&MI_01
%SPRD.CM4LOG% = Serial_Inst, USB\VID_1782&PID_000B&MI_02
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_000B&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_000C&MI_02
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_000C&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D00&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D00&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D01&MI_00
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D01&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D02&MI_01

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D03&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D03&MI_00
%SPRD.CPLOG%  = Serial_Inst, USB\VID_1782&PID_3D03&MI_03

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_3D10&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_3D13

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4001&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4001&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4001&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4001&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4001&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4001&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4001&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4002&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4002&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4002&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4002&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4002&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4002&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4002&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4003&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4003&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4003&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4004&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4004&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4004&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4004&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4004&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4004&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4004&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4012&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4012&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4012&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4012&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4012&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4012&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4012&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4013&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4013&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4013&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4015&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4015&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4015&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4015&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4015&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4015&MI_09


%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4022&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4022&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4022&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4022&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4022&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4022&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_4022&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4023&MI_03
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4023&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4023&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4024&MI_00
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_01
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_4024&MI_02
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4024&MI_03
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_04
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_4024&MI_05
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_4024&MI_06
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_4024&MI_07

;%SPRD.DIAG%  = Serial_Inst, USB\VID_1782&PID_4025&MI_03
;%SPRD.LOG%   = Serial_Inst, USB\VID_1782&PID_4025&MI_04
;%SPRD.AT%    = Serial_Inst, USB\VID_1782&PID_4025&MI_05

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4026&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4026&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4026&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4027&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4027&MI_03
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4027&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4028&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4028&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4029&MI_02

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4030&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4030&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4030&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4031&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4031&MI_03
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4031&MI_05

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4032&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4032&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4033&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4034&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4034&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4034&MI_05

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4035&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4035&MI_03
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4035&MI_05

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4036&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4036&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4037&MI_02

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4038&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4038&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4038&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4038&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4039&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4039&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4039&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4039&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4040&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4040&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4040&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4040&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4041&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4041&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4041&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_08
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4041&MI_09

%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4042&MI_08


%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4044&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4044&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4044&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4044&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4044&MI_08

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4045&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4045&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4045&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4045&MI_06
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4045&MI_07

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4046&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4046&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4046&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4046&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4047&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4047&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4047&MI_05

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4048&MI_03
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4048&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4048&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4048&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4048&MI_08

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4049&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4049&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4049&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4049&MI_06
%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4049&MI_07

%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4050&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4050&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4050&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4050&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4051&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4051&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4051&MI_05

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4052&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4052&MI_04
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4052&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4052&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4052&MI_08

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4053&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4053&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4053&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4053&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4053&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4054&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4054&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4054&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4054&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4055&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4055&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4055&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4056&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4056&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4056&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4056&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4057&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4057&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4057&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4057&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4058&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4058&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4058&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4058&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4059&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4059&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4059&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_07
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4059&MI_08

%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4060&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4061&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4061&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4061&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4061&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4061&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4062&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4062&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4062&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4062&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4063&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4063&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4063&MI_05

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4064&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4064&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4064&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4064&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4064&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4065&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4065&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4065&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4065&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4066&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4066&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4066&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4066&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4066&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4067&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4067&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4067&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4067&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4068&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4068&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4068&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4068&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4068&MI_07

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4069&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4069&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4069&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4069&MI_06

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4070&MI_00
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4070&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4070&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4070&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4070&MI_04

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4071&MI_00
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4071&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4071&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4071&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4072&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4072&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4072&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4073&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4073&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4073&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4073&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4073&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4073&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4073&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4074&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4074&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4074&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4074&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4074&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4074&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4075&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4075&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4075&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4075&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4075&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4076&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4076&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4076&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4076&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4076&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4076&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4076&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4077&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4077&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4077&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4077&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4077&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4077&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4078&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4078&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4078&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4078&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4078&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4078&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4078&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4079&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4079&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4079&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4079&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4079&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4079&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4080&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4080&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4080&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4080&MI_06
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4080&MI_07
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4080&MI_08
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4080&MI_09

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4081&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4081&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4081&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4081&MI_06
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4081&MI_07
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4081&MI_08

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4082&MI_00
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4082&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4082&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4082&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4082&MI_04
%WCN.AT%        = Serial_Inst, USB\VID_1782&PID_4082&MI_05
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4082&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4083&MI_00
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4083&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4083&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4083&MI_03
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4083&MI_04
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4083&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4084&MI_00
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4084&MI_01
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4084&MI_02
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4084&MI_03
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4084&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4085&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4085&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4085&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4085&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4085&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4086&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4086&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4086&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4086&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4086&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4087&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4087&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4087&MI_05
%WCN.AT%         = Serial_Inst, USB\VID_1782&PID_4087&MI_06
%WCN.DIAG%	   = Serial_Inst, USB\VID_1782&PID_4087&MI_07

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4088&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4088&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4088&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4088&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4088&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4089&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4089&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4089&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4089&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4090&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4090&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4090&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4091&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4091&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4091&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4091&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4091&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4092&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4092&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4092&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4092&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4093&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4093&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4093&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4094&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4094&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4094&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4094&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4094&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4095&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4095&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4095&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4095&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4096&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4096&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4096&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4097&MI_02
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4097&MI_03
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4097&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4097&MI_05
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4097&MI_06

%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4098&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4098&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4098&MI_04
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4098&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4099&MI_02
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4099&MI_03
%SPRD.AT2%     = Serial_Inst, USB\VID_1782&PID_4099&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4100&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4100&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4100&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4100&MI_0D

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4101&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4101&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4101&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4101&MI_0D

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4102&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4102&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4102&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4102&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4103&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4103&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4103&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4103&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4104&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4104&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4104&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4104&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4105&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4105&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4105&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4105&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4106&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4106&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4106&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4106&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4107&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4107&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4107&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4107&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4108&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4108&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4108&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4108&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4109&MI_08
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4109&MI_09
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4109&MI_0A
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4109&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410A&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410A&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410A&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410A&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410B&MI_06
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410B&MI_07
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410B&MI_08
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410B&MI_0A

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410C&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410C&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410C&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410C&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410D&MI_04
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410D&MI_05
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410D&MI_06
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410D&MI_08

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410E&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410E&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410E&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410E&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_410F&MI_02
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_410F&MI_03
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_410F&MI_04
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_410F&MI_06

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_4110&MI_00
%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4110&MI_01
%SPRD.LOG%     = Serial_Inst, USB\VID_1782&PID_4110&MI_02
%WCN.AT%       = Serial_Inst, USB\VID_1782&PID_4110&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4110&MI_04

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4111&MI_00
%WCN.AT%       = Serial_Inst, USB\VID_1782&PID_4111&MI_01
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_4111&MI_02

%SPRD.DIAG%     = Serial_Inst, USB\VID_1782&PID_4112&MI_00
%SPRD.AT%       = Serial_Inst, USB\VID_1782&PID_4112&MI_01
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4112&MI_02
%SPRD.AT2%       = Serial_Inst, USB\VID_1782&PID_4112&MI_03

%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_4D00

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4D01&MI_01
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4D01&MI_02

%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_4D02        ; For RDA

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_4D03&MI_00
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_4D03&MI_01

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5A5B&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5A5B&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5A5B&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5A5B&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5A5B&MI_09

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D03&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D03&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_05
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D03&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_07
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D03&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D03&MI_09

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D04&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D04&MI_03

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_5D06&MI_01
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D06&MI_02

%SPRD.DIAG%   = Serial_Inst, USB\VID_1782&PID_5D07&MI_01
%SPRD.LOG%    = Serial_Inst, USB\VID_1782&PID_5D07&MI_02
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D07&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D21&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D21&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D21&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D21&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D21&MI_0B

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D23&MI_02

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D24&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D24&MI_05
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_06
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D24&MI_07
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_08
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D24&MI_09
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_5D24&MI_0A
;8830ec
%TD.AT%       = Serial_Inst, USB\VID_1782&PID_5D25&MI_03
%TD.DIAG%     = Serial_Inst, USB\VID_1782&PID_5D25&MI_04
%W.AT%        = Serial_Inst, USB\VID_1782&PID_5D25&MI_05
%W.DIAG%      = Serial_Inst, USB\VID_1782&PID_5D25&MI_06
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D25&MI_07
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D25&MI_08
;8830ec
%TD.AT%       = Serial_Inst, USB\VID_1782&PID_5D26&MI_01
%TD.DIAG%     = Serial_Inst, USB\VID_1782&PID_5D26&MI_02
%W.AT%        = Serial_Inst, USB\VID_1782&PID_5D26&MI_03
%W.DIAG%      = Serial_Inst, USB\VID_1782&PID_5D26&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D26&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D26&MI_06
;Dechen8830
%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D27&MI_02
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D27&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D27&MI_04
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D27&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D28&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D28&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D28&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D28&MI_04

%USBCOMM_DL%  = Serial_Inst, USB\VID_1782&PID_5D29&MI_00

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D31&MI_03
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D31&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D31&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_5D34&MI_02
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D34&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D34&MI_04

%CUSPORT%     = Serial_Inst, USB\VID_1782&PID_5D38&MI_00

%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_01
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_5D39&MI_02
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_5D39&MI_03
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_04
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_5D39&MI_05
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_5D39&MI_06
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_5D39&MI_07

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_6000&MI_01
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_6000&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_6000&MI_03

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A002&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A002&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A002&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A002&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A002&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A002&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A002&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A012&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A012&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A012&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A012&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A012&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A012&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A012&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_A022&MI_04
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_05
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_A022&MI_06
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_A022&MI_07
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_08
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_A022&MI_09
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_A022&MI_0A
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_A022&MI_0B
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_A022&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_04
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_05
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_AD21&MI_06
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_AD21&MI_07
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_08
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_AD21&MI_09
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_0A
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_AD21&MI_0B
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_AD21&MI_0C

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_03
%COMDIAG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_AD24&MI_05
%WCN.DIAG%    = Serial_Inst, USB\VID_1782&PID_AD24&MI_06
%SPRDLOG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_07
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_AD24&MI_08
%LTEDIAG%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_09
%LTELOG%      = Serial_Inst, USB\VID_1782&PID_AD24&MI_0A
%SPRD.IQ%     = Serial_Inst, USB\VID_1782&PID_AD24&MI_0B

%SPRD.AT%     = Serial_Inst, USB\VID_1782&PID_D003&MI_01
%LTEAT%       = Serial_Inst, USB\VID_1782&PID_D003&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_1782&PID_D003&MI_03
%CUSPORT%     = Serial_Inst, USB\VID_1782&PID_D003&MI_04

;GOOGLE
%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D06&MI_03
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D06&MI_04
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D06&MI_05

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D07&MI_02
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D07&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D07&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_2D08&MI_02
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_2D08&MI_03
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_2D08&MI_04

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_01
%COMDIAG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_03
%WCN.DIAG%    = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_04
%SPRDLOG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_05
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_06
%LTEDIAG%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_07
%LTELOG%      = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_08
%SPRD.IQ%     = Serial_Inst, USB\VID_18D1&PID_4EE7&MI_09

%SPRD.AT%     = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_01
%LTEAT%       = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_02
%WCN.AT%      = Serial_Inst, USB\VID_18D1&PID_4EE8&MI_03

; LSD add start
%LSD.DIAG%   = Serial_Inst, USB\VID_3505&PID_1001&MI_02
%LSD.LOG%    = Serial_Inst, USB\VID_3505&PID_1001&MI_03
%LSD.AT%     = Serial_Inst, USB\VID_3505&PID_1001&MI_04
%LSD.DIAG%   = Serial_Inst, USB\VID_3505&PID_1002&MI_02
%LSD.LOG%    = Serial_Inst, USB\VID_3505&PID_1002&MI_03
%LSD.AT%     = Serial_Inst, USB\VID_3505&PID_1002&MI_04
%LSD.APLOG%  = Serial_Inst, USB\VID_3505&PID_1002&MI_06

; LCAT1 EC618/EC718
%LCAT1.AT%     = Serial_Inst, USB\Class_ff&SubClass_00&Prot_03
%LCAT1.LOG%    = Serial_Inst, USB\Class_ff&SubClass_00&Prot_04
%LCAT1.OPAQ%   = Serial_Inst, USB\Class_ff&SubClass_00&Prot_06

%LCAT1.QDLOADE% = Serial_Inst, USB\VID_17D1&PID_0001&REV_0200
; LSD add end

[Serial_Inst]
CopyFiles   = Serial.CopyFiles
AddReg      = Serial_Inst.AddReg

[Serial_Inst.AddReg]
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Serial_Inst.HW]
AddReg = Models_HW_AddReg

[Serial.CopyFiles]
sprdvcom.sys

[Serial_Inst.Services]
AddService=sprdvcom,0x00000002,Serial_Service 

[Serial_Service]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\sprdvcom.sys
AddReg         = Serial_Parameters_AddReg

[Models_HW_AddReg]
HKR,,DeviceCharacteristics,0x10001,0x0100         ; Use same security checks on relative opens
HKR,,Security,,"D:P(A;;GA;;;BA)(A;;GA;;;WD)"      ; Allow generic-all access to Built-in administrators and Local system 
HKR,,"VendorRequestTimeoutValue", %REG_DWORD%,5
HKR,,"SprdVendorRequest",%REG_DWORD%,1            ; If SprdVendorRequest is 1, CdcControlLineState will be ignored
HKR,,"CdcControlLineState",%REG_DWORD%,0          ; Only if SprdVendorRequest is 0, this configure will be worked
HKR,,"UseContinuousRead",%REG_DWORD%,0
HKR,,"RxFifoSize",%REG_DWORD%,128                 ; KByte
HKR,,"BulkInBufSize",%REG_DWORD%,4                ; KByte
HKR,,"UsbEnableZLP",%REG_DWORD%,1

[Serial_Parameters_AddReg]

;-------------- WDF Coinstaller installation

[Serial_Inst.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
WdfCoInstaller01009.dll

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[Serial_Inst.Wdf]
KmdfService = sprdvcom, Serial_wdfsect

[Serial_wdfsect]
KmdfLibraryVersion = 1.9

[Strings]
SPRD            = "UNISOC Communications Inc."
USBCOMM_DL      = "SPRD U2S Diag"
SPRD.AT         = "SPRD AT"
SPRD.DIAG       = "SPRD DIAG"
SPRD.LOG        = "SPRD LOG"
SPRD.IQ         = "SPRD IQ"
SPRD.CPLOG      = "SPRD CP LOG"
SPRD.AT2        = "SPRD Common AT"
SPRD.CM4LOG     = "SPRD WCN LOG"
COMDIAG         = "SPRD DIAG(SENSOR HUB)"
SPRDLOG         = "SPRD LOG(AGDSP)"
LTEAT           = "SPRD LTE AT(WIQ)"
LTEDIAG         = "SPRD LTE DIAG"
LTELOG          = "SPRD LTE LOG"
TD.AT           = "SPRD TD AT"
TD.DIAG         = "SPRD TD DIAG"
W.AT            = "SPRD WCDMA AT"
W.DIAG          = "SPRD WCDMA DIAG"
WCN.AT          = "SPRD WCN AT"
WCN.DIAG        = "SPRD WCN DIAG(LOG)"
DISK_NAME       = "UNISOC USB to Serial Install Disk"
CUSPORT			= "Customer Port"
REG_EXPAND_SZ   = 0x00020000 
REG_DWORD       = 0x00010001 

; LSD add start
LSD.DIAG   = "LSD USB DIAG Port"
LSD.LOG    = "LSD USB LOG Port"
LSD.AT     = "LSD USB AT Port"
LSD.APLOG  = "LSD USB AP LOG Port"

LCAT1.LOG   = "Lierda Log Port"
LCAT1.AT    = "Lierda At Port"
LCAT1.OPAQ  = "Lierda Uart Port"
LCAT1.QDLOADE = "Lierda QDLoade Port"
; LSD add end

